




JUMP JMP




CALL






Methods of looping



(used in digital watch, internet , traffic light.. where u need infinite loop, till the power is on of device)

JNZ

 (max count using 8 bit register is 255+1, 256 when we initialize the count by 00 H, focus to understand) (always put count above the loop outside, and DEC always in the last of the loop, because it affects the Zero Flag)

LOOP

